
Definitions

**RotoLock Mechanism**

Our unique RotoLock Mechanism feature can be incorporated into many of our products. The RotoLock Mechanism allows a housing or adapter to be attached to the front cover of a ring style or ringless meter socket, without the need to remove the cover by turning a centrally located activator. Once the electric meter is installed, the activator becomes inaccessible.



200 AMP




Ringless Style

Meter Socket

Activator

Head Unit/ Meter Socket Adapter

Lock Bars



(3 Locations)

Lock bar extended

6

[www.aeproducts.net](http://www.aeproducts.net/)